


35kv no breakdown




38kv breakdown




-45kv




-55kv



55 kv with surge arrestor



-45 kv with breakdown 10mm



-55kv 10mm

